{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["Head","Input","Output","Key figures","Change log","Evaluation","Lists, etc.","Intro","BaseIDs","Parameters and examples"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":1,"defined_names":141,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Head","index":0,"n_rows":22,"n_cols":3,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[null,20260219]
[]
[]
["General project information (Head section)"]
[]
["Path, energyPRO:","C:\\Program Files\\EMD\\energyPRO 5.1\\energyPRO.exe"]
["Project file, xml file and reports in same path as spreadsheet:","yes"]
["Name, project file:"]
["Path, project file:","C:\\work\\"]
["Path, xml file:","C:\\work\\"]
["Path, report files:","C:\\work\\"]
["Name, xml file:","input"]
["Calculate:","True"]
["Spool:","False"]
["Save:","True",true]
["SaveAs:"]
["Logging info and error messages","OnlyLogging"]
["Path, log files","C:\\work\\"]
["Date",{"$f":"NOW()","v":"2026-02-19T12:59:43.370"}]
["Version","1"]
["Language of Evaluation reports","English"]
["Currency format","#,##0.00 €"]

{"sheet":"Input","index":1,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Modifying input (input section)"]
[]
["Start run number",1]
["End run number",1]
["Input ID"]
["Data element"]
["Sub data element"]
["COMPARE, name of alternative"]
["Parameter name (corresponding to name in the energyPRO model)"]
["Resource"]
["Time series file type"]
["File field delimiter"]
["Data element index"]
[1,{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0},{"$f":"VLOOKUP(p_run,RunTable[],COLUMN())","v":0}]
["Present calculation:↗"]
["Run","Parameter 1","Parameter 2","Parameter 3","Parameter 4","Parameter 5","Parameter 6","Parameter 7","Parameter 14"]
[1]
[2]
[3]
[4]
[5]
[6]

{"sheet":"Output","index":2,"n_rows":17,"n_cols":1,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Requested reports (output section)"]
[]
["Output Report Type"]
["Report ID"]
["COMPARE, name of alternative"]
["Report name"]
["Report year"]
["Report extension"]
["Report delimiter"]
["Report decimal separator"]
["Report Resolution"]
["Report start date"]
["Report end date"]
["Report resource"]

{"sheet":"Key figures","index":3,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
["Report #"]
["row"]
["item"]
[]
[null,"2017-11-10T11:10:17"]
["Run","Column1","Column2","Column3","Column4","Column5","Column6","Column7","Column8","Column9"]
[1]
[2]
[3]
[4]
[5]
[6]

{"sheet":"Change log","index":4,"n_rows":22,"n_cols":2,"rows_kept":22,"cut":false,"hidden":true,"merged":[]}
[]
["2020-05-07","Including ExtendTSDays in Project identification"]
["2020-05-11","Including UseMilpSolver in Project identification"]
["2020-05-12","Including MilpChcRation and MilpMaxSec in Project identification"]
["2020-05-19","Fixing error in Collate_keyfigures sub."]
["2020-06-17","Changing solar unit values to include Ex"]
["2020-06-23","Find project file has been made more robust to drives without assigned letter"]
["2020-06-30","+ button for adding outputs and key figures"]
["2021-02-05","Reading csv file, the ReportDelimiter has been changed to DataDelimiter"]
["2022-03-08","Missing some logging, incl rebuilding to 4.8 with more fuels and more userfriendly strings"]
["2022-03-08","Adding a space to Demand to avoid duplicated Demand"]
["2022-03-18","When modifying power curves, it is evaluated if they shall be treated as formulas"]
["2022-03-23","Fixing issue with setting alternatives in outputs"]
["2022-04-19","Fixing issue with selecting graphic reports other than production graphic"]
["2022-05-10","Including hydraulic settings"]
["2022-07-07","Minor changes"]
["2022-10-07","Changed InsulationThickness to IsolationThichness"]
["2023-03-23","Changed action when run the Shell command is blocked, now comes a message on doing from energyPRO"]
["2024-08-19","Included built-in electrolyzer"]
["2024-10-09","Able to read .eppx"]
["2024-12-17","Include investment and disbursement"]
["2025-04-02","SaveAs saves as .eppx"]

{"sheet":"Evaluation","index":5,"n_rows":2,"n_cols":6,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
["Report","Parameter","Unit/Key Figure","Additional Input","Site","Comments"]

{"sheet":"Lists, etc.","index":6,"n_rows":296,"n_cols":15,"rows_kept":296,"cut":false,"hidden":true,"merged":[]}
[null,"Input types","Dataelements",null,"<?xml version=\"1.0\"?>",null,null,null,null,null,"XML-values:","Input types"]
[null,"Calculation Setup","ProjectIdentificationData","BaseID",null,null,null,null,null,null,null,"ProjectIdentificationData"]
[null,"Project Setup","ExternalConditionData","BaseID",null,null,null,null,null,null,null,"ExternalConditionData"]
[null,"Time Series","TimeSeriesData","BaseID",null,null,null,null,null,null,null,"TimeSeriesData"]
[null,"Time Series Function","TimeSeriesFunctionData","BaseID",null,null,null,null,null,null,null,"TimeSeriesFunctionData"]
[null,"Index","IndexData","BaseID",null,null,null,null,null,null,null,"IndexData"]
[null,"Site","SiteData","BaseID",null,null,null,null,null,null,null,"SiteData"]
[null,"Transmission","TransmissionData","BaseID",null,null,null,null,null,null,null,"TransmissionData"]
[null,"Resource","FuelData","BaseID",null,null,null,null,null,null,null,"FuelData"]
[null,"Demand","DemandData","BaseID",null,null,null,null,null,null,null,"DemandData"]
[null,"Energy Conversion Unit","EnergyConversionUnitData","BaseID",null,null,null,null,null,null,null,"EnergyConversionUnitData"]
[null,"Storage","StorageData","BaseID",null,null,null,null,null,null,null,"StorageData"]
[null,"Environment","EnvironmentData","BaseID",null,null,null,null,null,null,null,"EnvironmentData"]
[null,"Economy","EconomyData","BaseID",null,null,null,null,null,null,null,"EconomyData"]
[null,"Financing","FinancingData","BaseID",null,null,null,null,null,null,null,"FinancingData"]
[null,"Investment","InvestmentData","BaseID",null,null,null,null,null,null,null,"InvestmentData"]
[null,"Taxation","TaxationData","BaseID",null,null,null,null,null,null,null,"TaxationData"]
[null,"Project File","ProjectFile","Head",null,null,null,null,null,null,null,"ProjectFile"]
[]
[null,null,null,"DataName","AltName"]
[null,"Calculation Setup",null,null,null,null,null,null,null,null,null,"Project Identification"]
[null,"Project indentification comment",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"ID.Strings"]
[null,"Length of calculation step",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"CalcPeriodlengthMinutes"]
[null,"Length of optimisation period",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"OptimizationPeriodLength"]
[null,"Use MILP Solver",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"UseMilpSolver"]
[null,"MILP wanted precision",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"MilpCbcRatio"]
[null,"MILP Max solution time",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"MilpMaxSec"]
[null,"Extend TS, in days",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"ExtendTSDays"]
[]
[]
[null,"Project Setup",null,null,null,null,null,null,null,null,null,"ExternalConditionData"]
[null,"Calculation Start",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"CalcStart"]
[null,"Calculation End",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"CalcEnd"]
[]
[]
[null,"Time Series",null,null,null,null,null,null,null,null,null,"TimeSeriesData"]
[null,"TimeSeries",null,"DataElementName","TimeSeriesFileName","TimeSeriesFileTypes",null,null,null,null,null,"Weatherdata.TimeSeries"]
[null,"Is In Daylight Saving",null,"DataElementName","DataElementValue","txt",null,null,"TimeSeriesFileType",null,null,"IsInDaylightSaving"]
[null,"Latitude",null,"DataElementName","DataElementValue","csv",null,null,"DataDelimiter",null,null,"Latitude"]
[null,"Longitude",null,"DataElementName","DataElementValue","epw",null,null,null,null,null,"Longitude"]
[null,"Developing over the years",null,"DataElementName","DataElementValue","xml",null,null,null,null,null,"DevelopingFlag"]
[]
[]
[null,"Time Series Function",null,null,null,null,null,null,null,null,null,"TimeSeriesFunctionData"]
[null,"Function",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"FuncFormular"]
[null,"Latitude",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"Latitude"]
[null,"Longitude",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"Longitude"]
[null,"Unit",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"WeatherUnit"]
[]
[null,"Index",null,null,null,null,null,null,null,null,null,"IndexData"]
[null,"Index Data Time Series",null,"DataElementName","TimeSeriesFileName",null,null,null,null,null,null,"IndexData.TimeSeries"]
[]
[null,"Fuel",null,null,null,null,null,null,null,null,null,"FuelData"]
[null,"Heat Value",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"ThermalValue"]
[null,"Ressource unit",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"UnitName"]
[]
[]
[null,"Site",null,null,null,null,null,null,null,null,null,"SiteData"]
[null,"Minimum Required Heat Supply Temperature",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"RequiredSupplyTempMin"]
[null,"Minimum Delivered Heat Return Temperature",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"DeliveredReturnTempMin"]
[]
[null,"Transmission",null,null,null,null,null,null,null,null,null,"TransmissionData"]
[null,"Site A can transmit to site B",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"SiteAtoB"]
[null,"Site B can transmit to site A",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"SiteBtoA"]
[null,"Capacity",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"Capacity"]
[null,"Loss",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"Loss"]
[null,"Length of Transmission",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"LengthOfTransmission"]
[null,"Internal Diameter",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"InternalDiameter"]
[null,"Pipe Roughness",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"PipeRoughness"]
[null,"Specific Heat Loss",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"SpecificHeatLoss"]
[null,"Max Velocity",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"MaxVelocity"]
[null,"Max Pressure Gradient",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"MaxPressureGradient"]
[null,"Ground Temperature",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"GroundTempEx","GroundTemp","UseGroundTempEx"]
[null,"Non Available Periods, Start",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"NonAvailableTimes.StartTime"]
[null,"Non Available Periods, End",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"NonAvailableTimes.EndTime"]
[null,"Non Available Periods, Occurrence",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"NonAvailableTimes.Occurrence"]
[null,"Operational From",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"OperationalFrom"]
[null,"Operational To",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"OperationalTo"]
[]
[]
[null,"Demand",null,null,null,null,null,null,null,null,null,"DemandData"]
[null,"Demand ",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"Demand"]
[null,"Symbol for ambient temperature",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"OutDoorTempSymbol"]
[null,"Reference Temperature",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"ReferenceTemperature"]
[null,"Dependent Fraction",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"WeatherDepFraction"]
[null,"Restricted Season, From",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"WeatherDepSeasonFrom"]
[null,"Restricted Season, To",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"WeatherDepSeasonTo"]
[null,"Fixed Profile",null,"DataElementName","TimeSeriesFileName",null,null,null,null,null,null,".FixedProfile"]
[null,"Restricted period, From",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"IncludedFrom"]
[null,"Restricted period, To",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"IncludedTo"]
[null,"Site",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"SiteID"]
[null,"Demand Time Series",null,"DataElementName","TimeSeriesFileName",null,null,null,null,null,null,"Weatherdata.TimeSeries"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"XML-values:"]
[null,"Energy Conversion Unit","Sub dataelements",null,null,"PowerCurveElements",null,null,null,null,"OccurrenceElements","EnergyConversionUnitData","PowerCurveElements",null,"Use"]
[null,"Power curve","PowerCurveElements","DataElementName","DataElementValue","Input",null,null,"DataElementValue",null,"once","PowerCurve","EtypeInput.ValueEX","EtypeInput.Value","EtypeInput.UseEX"]
[null,"Solar","SolarUnitElements","DataElementName","DataElementValue","Output",null,null,"DataElementValue",null,"yearly","SolarUnit","EtypeOutput.ValueEX","EtypeOutput.Value","EtypeOutput.UseEX"]
[null,"Wind Farm","WindFarmElements","DataElementName","DataElementValue",null,null,null,null,null,"monthly","WindFarm"]
[null,"Heat Pump","HeatPumpElements","DataElementName","DataElementValue",null,null,null,null,null,"weekly","HeatPump"]
[null,"Rejection","RejectionElements","DataElementName","DataElementValue",null,null,null,null,null,"daily","RejectionData"]
[null,"Electrolyzer","ElectrolyzerElements","DataElementName","DataElementValue",null,null,null,null,null,null,"Electrolyzer"]
[null,"Non Available Periods, Start",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"NonAvailableTimes.StartTime"]
[null,"Non Available Periods, End",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"NonAvailableTimes.EndTime"]
[null,"Non Available Periods, Occurrence",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"NonAvailableTimes.Occurrence"]
[null,"Operational From",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"OperationalFrom"]
[null,"Operationa lTo",null,"DataElementName","DataElementTimeValue",null,null,null,null,null,null,"OperationalTo"]
[null,"Starting Up Period",null,"DataElementName","DataElementValue","Fuel Input (4.8 and higher)",null,null,"DataElementEnergyType",null,null,"StartUpPeriod"]
[null,"Shutting Down Period",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"ShutDownPeriod"]
[null,"Minimum Operating Hours",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"MinimumOperatingTime"]
[null,"Minimum Non Operating Hours",null,"DataElementName","DataElementValue","SolarUnitElements",null,null,null,null,null,"MinimumNonOperatingTime","SolarUnitElements"]
[null,null,null,null,null,"Total Area",null,null,"DataElementValue",null,null,null,"TotalArea"]
[null,"Storage",null,null,null,"Inclination",null,null,"DataElementValue",null,null,"StorageData","InclinationEx"]
[null,"Storage Volume",null,"DataElementName","DataElementValue","Orientation",null,null,"DataElementValue",null,null,"StorageVolume","OrientationEX"]
[null,"Temperature In The Top",null,"DataElementName","DataElementValue","N0",null,null,"DataElementValue",null,null,"TempTop","N0"]
[null,"Temperature In The Bottom",null,"DataElementName","DataElementValue","K0",null,null,"DataElementValue",null,null,"TempBottom","K0"]
[null,"Storage Utilization",null,"DataElementName","DataElementValue","K1",null,null,"DataElementValue",null,null,"StorageUtilization","K1"]
[null,"Minimum Storage Capacity in Pct",null,"DataElementName","DataElementValue","Incidence Angle Modifier at 50 deg.",null,null,"DataElementValue",null,null,"MinStorageCapPct","IncidenceAngleMod50"]
[null,"Storage Height",null,"DataElementName","DataElementValue","Incidence Angle Mod Coefficient",null,null,"DataElementValue",null,null,"StorageHeight","IncidenceAngleModCoef"]
[null,"Insulation Thickness",null,"DataElementName","DataElementValue","Installed Electric Capacity",null,null,"DataElementValue",null,null,"IsolationThichness","InstalledElecCapacity"]
[null,"Thermal Conductivity",null,"DataElementName","DataElementValue","Maximum Power",null,null,"DataElementValue",null,null,"ThermalConductivity","PMaxEx"]
[null,"Ambient Temperature",null,"DataElementName","DataElementValue","Temperature Coefficient",null,null,"DataElementValue",null,null,"AmbientTemperature","TempCoeffPowerEx"]
[null,"Pumped Hydro, Height Difference",null,"DataElementName","DataElementValue","NOCT",null,null,"DataElementValue",null,null,"HeightDiff","NOCTEx"]
[null,"Water Reservoir Max",null,"DataElementName","DataElementValue","Losses from module to grid",null,null,"DataElementValue",null,null,"WaterReservoirMax","PowerLossesEx"]
[null,"Pumping Power Capacity",null,"DataElementName","DataElementValue","Percent Losses In Pipes",null,null,"DataElementValue",null,null,"PumpPowerCapacity","PercentLossInPipes"]
[null,"Pumping Power Efficiency",null,"DataElementName","DataElementValue","Temperature From Collector",null,null,"DataElementValue",null,null,"PumpPowerEfficiency","ForwardTemperature"]
[null,"Producing Power Capacity",null,"DataElementName","DataElementValue","Temperature To Collector",null,null,"DataElementValue",null,null,"PumpProdCapacity","ReturnTemperature"]
[null,"Producing Power Efficiency",null,"DataElementName","DataElementValue","Temperature On Demand Side",null,null,"DataElementValue",null,null,"PumpProdEfficiency","TempOnDemandSide"]
[null,"Max Capacity",null,"DataElementName","DataElementValue","Number Of Rows",null,null,"DataElementValue",null,null,"MaxCapacityEX","NumberOfRows"]
[null,"EVs Capacity",null,"DataElementName","DataElementValue","Inclination Ground",null,null,"DataElementValue",null,null,"ECarsCapacityEX","InclinationGround"]
[null,"Charging Capacity",null,"DataElementName","DataElementValue","Distance Between Rows",null,null,"DataElementValue",null,null,"InletCapacity","DistanceBetweenRows"]
[null,"Discharging Capacity",null,"DataElementName","DataElementValue","Orientation Ground",null,null,"DataElementValue",null,null,"OutletCapacity","OrientationGround"]
[null,"Charging Efficiency",null,"DataElementName","DataElementValue","Height Solar Unit",null,null,"DataElementValue",null,null,"InletEfficiency","SolarUnitHeight"]
[null,"Discharging Efficiency",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"OutletEfficiency"]
[]
[null,null,null,null,null,"WindFarmElements",null,null,null,null,null,null,"WindFarmElements"]
[null,"Environment",null,null,null,"Annual Production",null,null,"DataElementValue",null,null,"EnvironmentData","AnnualProduction"]
[null,"Amount Per Unit",null,"DataElementName","DataElementValue","Windspeed Time series",null,null,"DataElementValue",null,null,"Amount","WindTSID"]
[null,null,null,null,null,"Measure Height",null,null,"DataElementValue",null,null,null,"MeasureHeight"]
[null,null,null,null,null,"Hub Height",null,null,"DataElementValue",null,null,null,"HubHeight"]
[null,"Economy",null,null,null,"Scale Type",null,null,"DataElementValue",null,null,"EconomyData","ScaleType"]
[null,"Price Per Unit",null,"DataElementName","DataElementValue","Scale Value",null,null,"DataElementValue",null,null,"Amount","ScaleValue"]
[null,"Nominal Discount Rate",null,"DataElementName","DataElementValue","Hellmann Exponent",null,null,"DataElementValue",null,null,"NominalDiscountRate","HellmannExp"]
[]
[]
[null,"Financing",null,null,null,"NonOperTimesElements",null,null,null,null,null,"FinancingData","NonOperTimesElements"]
[null,"Annual Interest",null,"DataElementName","DataElementValue","StartTime",null,null,"DataElementTimeValue",null,null,"AnnualInterest","StartTime"]
[null,"Disbursement",null,"DataElementName","DataElementValue","EndTime",null,null,"DataElementTimeValue",null,null,"FinancingData.Disbursement","EndTime"]
[null,"Loan Period Years",null,"DataElementName","DataElementValue","EndTime",null,null,"DataElementTimeValue",null,null,"LoanPeriodYears","EndTime"]
[null,"Loan Period Months",null,"DataElementName","DataElementValue","StartTime",null,null,"DataElementIndex",null,null,"LoanPeriodMonths","StartTime"]
[]
[null,"Investment",null,null,null,null,null,null,null,null,null,"InvestmentData"]
[null,"Amount",null,"DataElementName","DataElementValue",null,null,null,null,null,null,"InvestmentData.Investment"]
[]
[null,null,null,null,null,"HeatPumpElements",null,null,null,null,null,null,"HeatPumpElements"]
[null,"Taxation",null,null,null,"Electrical Capacity",null,null,"DataElementValue",null,null,"TaxationData","ElectricalCapacity"]
[null,"Tax Rate",null,"DataElementName","DataElementValue","Min. Electrical Capacity",null,null,"DataElementValue",null,null,"TaxRate","MinElecCapacity"]
[null,"Loss Carried Forward",null,"DataElementName","DataElementValue","Heat Output restricted to",null,null,"DataElementValue",null,null,"LossCarriedForward","MaxHeatCapacity"]
[null,null,null,null,null,"COP",null,null,"DataElementValue",null,null,null,"COP"]
[null,null,null,null,null,"Heated From",null,null,"DataElementValue",null,null,null,"HeatedFrom"]
[null,"Output Types",null,null,null,"Heated To",null,null,"DataElementValue",null,null,"Output Types","HeatedTo"]
[null,"Text report","OutputReports","TextReportFileTypes",null,"Cooled From",null,null,"DataElementValue",null,null,"Text report","CooledFrom"]
[null,"Graphic report","GraphicOutputReports","GraphicReportFileTypes",null,"Cooled To",null,null,"DataElementValue",null,null,"Graphic report","CooledTo"]
[null,null,null,null,null,"Actual temperatures Heated From",null,null,"DataElementValue",null,null,null,"HeatedFromExprStr"]
[null,null,null,null,null,"Actual temperatures Heated To",null,null,"DataElementValue",null,null,null,"HeatedToExprStr"]
[null,"Output Reports",null,null,"ReportFileTypes","Actual temperatures Cooled To",null,null,"DataElementValue",null,null,"Output Reports","CooledFromExprStr"]
[null,"Energy Conversion Annual",null,null,"txt","Actual temperatures Cooled From",null,null,"DataElementValue",null,null,"EnergyConversionAnnual","CooledToExprStr"]
[null,"Energy Conversion Monthly",null,null,"csv","Cut Off When Cooled Is Below",null,null,"DataElementValue",null,null,"EnergyConversionMonthly","CutOffWhenCooled"]
[null,"Energy Conversion Summary",null,null,"pdf",null,null,null,null,null,null,"EnergyConversionSummary"]
[null,"Environment Monthly",null,null,null,"RejectionElements",null,null,null,null,null,"EnvironmentMonthly","RejectionElements"]
[null,"Environment Summary",null,null,null,"Rejection Capacity",null,null,"DataElementValue",null,null,"Environment","BlowOffCapacity"]
[null,"Production Plan",null,"Output Report Type",null,"Electricity consumption",null,null,"DataElementValue",null,null,"ProductionPlan","ElecConsumption"]
[null,"Cash Flow Monthly",null,"Report ID","ReportBaseID","Electricity consumption in pct",null,null,"DataElementValue",null,null,"CashFlowMonthly","ElecConsumptionPct"]
[null,"Cash Flow Summary",null,"COMPARE, name of alternative","AltName",null,null,null,null,null,null,"CashFlowSummary"]
[null,"Operation Income/Cash flow Annual",null,"Report name","ReportFileName","ElectrolyzerElements",null,null,null,null,null,"OperationIncome","ElectrolyzerElements"]
[null,"Financial Key Figures",null,"Report year","ReportYear","Electric capacity",null,null,"DataElementValue",null,null,"FinancialKeyFigures","ElecToHydrogenEff"]
[null,"Income Statement",null,"Report extension","ReportFileType","Electricity to hydrogen efficiency",null,null,"DataElementValue",null,null,"IncomeStatement","ElectricCapacity"]
[null,"Income Statement Summary",null,"Report delimiter","ReportDelimiter","Heat_Output",null,null,"DataElementValue",null,null,"IncomeStatementSummary","HeatOutPutStr"]
[null,"Balance Sheet",null,"Report decimal separator","ReportDecimalSeparator","Minimal load",null,null,"DataElementValue",null,null,"BalanceSheet","MinimalElecLoad"]
[null,"Balance Sheet Summary",null,"Report Resolution","ReportResolution",null,null,null,null,null,null,"BalanceSheetSummary"]
[null,"Catalogue Technical Assumptions",null,"Report start date","ReportStartDate",null,null,null,null,null,null,"CatalogueTechnicalAssumptions"]
[null,"Catalogue Economic Assumptions",null,"Report end date","ReportEndDate",null,null,null,null,null,null,"CatalogueEconomicAssumptions"]
[null,"Operation Strategy Calculation",null,"Report resource","ReportResource",null,null,null,null,null,null,"OperationStrategyCalculation"]
[null,"Project Reports",null,null,null,"ReportFileType",null,null,null,null,null,"ProjectReports"]
[null,"Export Energy Conversion",null,null,"ReportResolution",null,null,null,null,null,null,"ToolsCopyEnergyConversion"]
[null,"Export Payments",null,null,"Year",null,null,null,null,null,null,"ToolsExportEconomy"]
[null,"Export Hydraulic transmissions",null,null,"Month",null,null,null,null,null,null,"ToolsCopyHydraulicTransmissions"]
[null,"Compare Energy Conversion",null,null,"Day",null,null,null,null,null,null,"CompareEnergyConversion"]
[null,"Compare Environment",null,null,"Hour",null,null,null,null,null,null,"CompareEnvironment"]
[null,"Compare CashFlow",null,null,"Step",null,null,null,null,null,null,"CompareCashFlow"]
[null,"Compare Income Statement",null,null,null,null,null,null,null,null,null,"CompareIncomeStatement"]
[null,"Compare Financial Key Figures",null,null,"Graphic ReportFileTypes",null,null,null,null,null,null,"CompareFinancialKeyFigures"]
[null,"Calculation Log",null,null,"jpg",null,null,null,null,null,null,"CalculationLog"]
[]
[]
[null,null,"ProductionGraphic"]
[null,"Graphic Output Reports",null,null,null,null,null,null,null,null,null,"Graphic Output Reports"]
[null,"Production Graphic",null,null,null,null,null,null,null,null,null,"ProductionGraphic"]
[null,"Transmission Graphic",null,null,null,null,null,null,null,null,null,"TransmissionGraphic"]
[null,"Duration Curve",null,null,null,null,null,null,null,null,null,"DurationCurve"]
[null,"Cash Flow Graphic",null,null,null,null,null,null,null,null,null,"CashFlowGraphic"]
[null,"Graphical Layout",null,null,null,null,null,null,null,null,null,"GraphicalLayout"]
[null,"Compare KeyFigures Net Present Value",null,null,null,null,null,null,null,null,null,"CompareKeyFiguresNetPresentValue"]
[null,"Compare KeyFigures Payback Time",null,null,null,null,null,null,null,null,null,"CompareKeyFiguresPayBackTime"]
[null,"Compare KeyFigures IRR",null,null,null,null,null,null,null,null,null,"CompareKeyFiguresIRR"]
[]
[]
[]
[]
[]
[null,"ProductionGraphic",null,null,null,null,null,null,null,null,null,"ProductionGraphic"]
[null,"ReportStartDate",null,null,null,null,null,null,null,null,null,"ReportStartDate"]
[null,"ReportEndDate",null,null,null,null,null,null,null,null,null,"ReportEndDate"]
[]
[]
[null,"Evaluation"]
[]
[]
[null,"Report types DE",null,"Report types Eng",null,"Report types DK",null,null,null,"Currency"]
[null,"Energieumwandlung, jährlich","energy_conversion","Energy conversion, annual","energy_conversion_eng","Energiomsætning, Årlig","energy_conversion_dk","German",null,"#,##0.00 €"]
[null,"Betriebsergebnis","operation_income","Operation income","operation_income_eng","Resultat af ordinær drift","operation_income_dk","English",null,"$ #,##0.00"]
[null,"Energieumwandlung, Zusammenfassung","energy_conversion_Sum","Energy conversion, summary","energy_conversion_Sum_eng","Energiomsætning, oversigt","energy_conversion_Sum_dk","Danish",null,"£ #,##0.00"]
[null,"Cash-Flow, Übersicht","cash_flow_sum","Cash-Flow, summary","cash_flow_sum_eng","Likviditetsbudget, Oversigt","cash_flow_sum_dk",null,null,"#,##0.00 \"DKK\""]
[]
[]
[]
[]
[]
[]
[]
[null,"Energieumwandlung",null,"Energy conversion",null,"Energiomsætning"]
[null,"Wärmelastgänge:",null,"Heat demands:",null,"Varmbehov:"]
[null,"Wärmeproduktion:",null,"Heat productions:",null,"Varmeproduktioner:"]
[null,"Kältebedarf:",null,"Cooling demands:",null,"Kølebehov:"]
[null,"Kälteproduktion:",null,"Cooling productions:",null,"Køleproduktioner:"]
[null,"Stromproduktion durch Energieanlagen:",null,"Electricity produced by energy units:",null,"Elektricitet produceret af energianlæg:"]
[null,"Strombedarf durch Energieanlagen:",null,"Electricity consumed by energy units:",null,"Elektricitet forbrugt af energianlæg:"]
[null,"Spitzenstromproduktion:",null,"Peak electric production:",null,"Peak elproduktion:"]
[null,"Stromaustausch:",null,"Electricity exchange:",null,"Elektricitetsudveksling:"]
[null,"Betriebsstunden:",null,"Hours of operation:",null,"Driftstimer:"]
[null,"Volllaststunden:",null,"Full load hours:",null,"Fuldlasttimer:"]
[null,"Starts:",null,"Starts:",null,"Starter:"]
[null,"Brennstoffe:",null,"Fuels:",null,"Brændsler:"]
[null,"Kennzahlen:",null,"Various key figures:",null,"Diverse noegletal:"]
[null,"Übertragungsverluste:",null,"Transmission losses:",null,"Transmissionstab:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Betriebsergebnis",null,"Operation income",null,"Resultat af ordinær drift"]
[null,"Betriebliche Einnahmen",null,"Revenues",null,"Driftsindtægter"]
[null,"Gesamt Betriebliche Einnahmen",null,"Total revenues",null,"Ialt Driftsindtægter"]
[null,"Betriebliche Aufwendungen",null,"Operating Expenditures",null,"Driftsudgifter"]
[null,"Gesamt Betriebliche Aufwendungen",null,"Total Operating Expenditures",null,"Ialt Driftsudgifter"]
[null,"Betriebsergebnis",null,"Operation income",null,"Resultat af ordinær drift"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Energieumwandlung, Zusammenfassung",null,"Energy conversion, summary",null,"Energiomsætning, oversigt"]
[null,"Wärmebedarf",null,"Heat demand",null,"Varmebehov"]
[null,"Stromproduktion durch Energieanlagen",null,"Electricity produced by energy units",null,"Elektricitet produceret af energianlæg"]
[null,"Stromeinspeisung",null,"Exported electricity",null,"Leveret elektricitet"]
[]
[]
[]
[]
[null,"Cash-Flow, Übersicht",null,"Cash flow, summary",null,"Likviditetsbudget, Oversigt"]
[null,"Betriebliche Einnahmen",null,"Revenues",null,"Driftsindtægter"]
[null,"Gesamt Betriebliche Einnahmen",null,"Total Revenues",null,"Ialt Driftsindtægter"]
[null,"Betriebliche Aufwendungen",null,"Operating Expenditures",null,"Driftsudgifter"]
[null,"Gesamt Betriebliche Aufwendungen",null,"Total Operating Expenditures",null,"Ialt Driftsudgifter"]
[null,"Investitionen",null,"Investments",null,"Investeringer"]
[null,"Finanzierung ...",null,"Cash From Long Term Financing",null,"Finansiering"]
[null,"Schuldendienst",null,"Debt service",null,"Ydelse og gebyr"]
[null,"Zinsen auf liquide Mittel",null,"Total Interest on Cash Account",null,"Ialt Likvidbeholdning, renter"]
[null,"Zahlungsmittelüberschuss",null,"Cash Surplus",null,"Tilvækst i likvidbeholdning"]
[null,"Liquide Mittel",null,"Cash Account",null,"Likvidbeholdning"]
[]
[]
[]
[null,"Starts",null,"Turn ons",null,"Starter"]
[null,"Vollbenutzungsstunden",null,"Full load operating hours",null,"Fuldlastsdriftstimer"]
[null,"Auslastungsgrad",null,"Utilization factor",null,"Udnyttelsesfaktor"]
[null,"Jahresnutzungsgrad",null,"Total efficiency",null,"Totaleffektivitet"]

{"sheet":"Intro","index":7,"n_rows":67,"n_cols":2,"rows_kept":67,"cut":false,"hidden":true,"merged":[]}
["Example of calling energyPRO by xml"]
[]
[]
["energyPRO is called with the following parameters:"]
["c:\\Program Files\\Emd\\energyPRO 4\\energyPRO4.exe /XMLMod c:\\example.xml"]
[]
["/XMLMod is telling energyPRO that this is by xml"]
["The last parameter is the xml-file."]
[]
["This is an example of the content of an xml-file."]
["energyPRODataFile refers to the energyPRO file, which is to be altered."]
["The input data elements refer to the elements in the energyPRO, which are to be changed. In this case the demand \"Ab værk leverance\" and the payment \"Motor 1\" in the "]
["payment group \"Nox-afgifter\"."]
["Three report files will be saved."]
["<?xml version=\"1.0\" encoding=\"UTF-8\"?>"]
["<XMLtoEnergyPRO> "]
["<Head> "]
[null,"<energyPRODataFile>c:\\energyPRO data\\Dansk\\Danske eksempler\\Vestdansk 5MW-kraftvarmeværk på markedsvilkår i 2011.epp</energyPRODataFile> "]
[null,"<Version>1</Version> "]
[null,"<Date>01-06-2011</Date> "]
[]
["</Head> "]
["<InputDataElements>"]
[]
["   <InputDataElement> "]
["      <BaseID>500</BaseID> "]
["      <DataName>Ab værk leverance</DataName> "]
["      <DataElementName>Demand</DataElementName> "]
["      <DataElementValue>40000</DataElementValue> "]
["   </InputDataElement> "]
[]
["    <InputDataElement>      "]
["      <BaseID>800</BaseID>"]
["      <DataName>NOx-afgifter.Motor 1</DataName>"]
["      <DataElementName>amount</DataElementName>"]
["      <DataElementValue>0.03</DataElementValue> "]
["   </InputDataElement>"]
[]
["</InputDataElements> "]
[]
["<OutputDataElements> "]
[]
["   <OutputDataElement>      "]
["      <ReportBaseID>200</ReportBaseID>"]
["      <ReportDelimiter>;</ReportDelimiter>"]
["      <ReportFileName>c:\\Energy conversion, annual.txt</ReportFileName>"]
["      <ReportFileType>txt</ReportFileType>"]
["   </OutputDataElement>   "]
[]
["   <OutputDataElement>      "]
["      <ReportBaseID>100</ReportBaseID>"]
["      <ReportFileName>c:\\production, graphic1.jpg</ReportFileName>"]
["      <ReportFileType>jpg</ReportFileType>"]
["      <ReportStartDate>15-07-2011 00:00</ReportStartDate>"]
["      <ReportEndDate>23-07-2011 00:00</ReportEndDate>"]
["   </OutputDataElement>   "]
[]
["   <OutputDataElement>      "]
["      <ReportBaseID>10030</ReportBaseID>"]
["      <ReportDelimiter>;</ReportDelimiter>"]
["      <ReportFileName>c:\\OperationIncome.csv</ReportFileName>"]
["      <ReportFileType>csv</ReportFileType>"]
["   </OutputDataElement>   "]
[]
["</OutputDataElements>"]
[" "]
["</XMLtoEnergyPRO>"]

{"sheet":"BaseIDs","index":8,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["InputData ","BaseID: ",100,"Project identification"]
["InputData ","BaseID: ",200,"External conditions"]
["InputData ","BaseID: ",205,"Time series"]
["InputData ","BaseID: ",210,"Time series functions","Not implemented"]
["InputData ","BaseID: ",215,"Indexes","Not implemented"]
["InputData ","BaseID: ",350,"Sites","Not implemented"]
["InputData ","BaseID: ",375,"Transmissions","Not implemented"]
["InputData ","BaseID: ",400,"Fuels"]
["InputData ","BaseID: ",500,"Demands"]
["InputData ","BaseID: ",600,"Energy conversion units"]
["InputData ","BaseID: ",650,"Storages"]
["InputData ","BaseID: ",690,"Electricity market"]
["InputData ","BaseID: ",700,"Operation strategy"]
["InputData ","BaseID: ",750,"Environment"]
["InputData ","BaseID: ",800,"Economy"]
["InputData ","BaseID: ",800,"Revenues"]
["InputData ","BaseID: ",800,"Operation expenditures"]
["InputData ","BaseID: ",840,"Investments"]
["InputData ","BaseID: ",850,"Financing"]
["InputData ","BaseID: ",860,"Taxation"]
["Reports ","BaseID: ",0,"Copy to clipboard"]
["Reports ","BaseID: ",100,"Production, graphic",null,null,null,"Graphical"]
["Reports ","BaseID: ",200,"Energy conversion, annual",null,null,null,"Text"]
["Reports ","BaseID: ",300,"Energy conversion, monthly"]
["Reports ","BaseID: ",350,"Energy conversion, summary"]
["Reports ","BaseID: ",400,"Duration curve for heat demand"]
["Reports ","BaseID: ",401,"Duration curve for process heat demand"]
["Reports ","BaseID: ",410,"Duration curve for electricity demand"]
["Reports ","BaseID: ",420,"Duration curve for cooling demand"]
["Reports ","BaseID: ",900,"Environment"]
["Reports ","BaseID: ",1000,"Production Plan"]
["Reports ","BaseID: ",10000,"Cash Flow, monthly"]
["Reports ","BaseID: ",10010,"Cash Flow, summary"]
["Reports ","BaseID: ",10020,"Cash flow, graphic"]
["Reports ","BaseID: ",10030,"Operation Income"]
["Reports ","BaseID: ",10040,"Financial Key Figures"]
["Reports ","BaseID: ",10060,"Income Statement"]
["Reports ","BaseID: ",10080,"Income Statement, summary"]
["Reports ","BaseID: ",10100,"Balance Sheet"]
["Reports ","BaseID: ",10110,"Balance Sheet, summary"]
["Reports ","BaseID: ",12000,"Catalogue of Technical Assumptions"]
["Reports ","BaseID: ",12100,"Catalogue of Economical Assumptions"]
["Reports ","BaseID: ",20000,"Operation Strategy Calculation"]
["Reports ","BaseID: ",20090,"Graphical Layout"]

{"sheet":"Parameters and examples","index":9,"n_rows":202,"n_cols":17,"rows_kept":202,"cut":false,"hidden":true,"merged":[]}
["ProjectIdentification",null,null,null,"Example"]
[null,"CalcPeriodLengthMinutes",null,null,"Modifying calculation step"]
[null,null,null,null,"   <InputDataElement> "]
[null,null,null,null,null,"<BaseID>100</BaseID> "]
[null,null,null,null,null,"<DataElementName>CalcPeriodLengthMinutes</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>15</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
[null,"OptimizationPeriodLength",null,null,"Modifying optimization period length"]
[null,null,null,null,"   <InputDataElement> "]
[null,null,null,null,null,"<BaseID>100</BaseID> "]
[null,null,null,null,null,"<DataElementName>OptimizationPeriodLength</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>oplYear</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
["External Conditions"]
[null,"CalcEnd",null,null,"Modifying calculation starttime"]
[null,null,null,null,"<InputDataElement>"]
[null,null,null,null,"<BaseID>200</BaseID>"]
[null,null,null,null,null,"<DataElementName>CalcStart</DataElementName>"]
[null,null,null,null,null,"<DataElementTimeValue>07-03-2000 00:00</DataElementTimeValue>"]
[null,null,null,null,"</InputDataElement>"]
[]
[null,"CalcStart",null,null,"Modifying calculation endtime"]
[null,null,null,null,"<InputDataElement>"]
[null,null,null,null,null,"<BaseID>200</BaseID>"]
[null,null,null,null,null,"<DataElementName>CalcEnd</DataElementName>"]
[null,null,null,null,null,"<DataElementTimeValue>14-03-2000 11:00</DataElementTimeValue>"]
[null,null,null,null,"</InputDataElement>"]
[]
["Time Series"]
[null,"TimeSeries",null,null,"Modifying time series by replacing with external file, here xml:",null,null,null,null,null,null,null,null,null,"xml data file:"]
[null,"File type:",null,null,"    <InputDataElement>      ",null,null,null,null,null,null,null,null,null,"<?xml version=\"1.0\" encoding=\"windows-1252\"?>"]
[null,"txt",null,null,null," <BaseID>205</BaseID>",null,null,null,null,null,null,null,null,"  <ePROTimeSeriesData>"]
[null,"csv",null,null,null,"<DataName>UdeTemp</DataName>"]
[null,"epw",null,null,null,"<DataElementName>weatherdata.TimeSeries</DataElementName>",null,null,null,null,null,null,null,null,"    <Head>"]
[null,"xml",null,null,null," <TimeSeriesFileName>c:\\temp\\xmltest\\Udetemp.xml</TimeSeriesFileName>",null,null,null,null,null,null,null,null,null,"<Date>28-10-2009  </Date>"]
[null,null,null,null,null,"<TimeSeriesFileType>xml</TimeSeriesFileType>",null,null,null,null,null,null,null,null,null,"<Filename>Atest-2 dage.xml </Filename>"]
[null,null,null,null,"   </InputDataElement>",null,null,null,null,null,null,null,null,null,"</Head>"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<TimeSeriesElement>"]
[null,null,null,null,"epw:",null,null,null,null,null,null,null,null,null,null,"<DataName>UdeTemp</DataName> "]
[null,null,null,null,"    <InputDataElement>      ",null,null,null,null,null,null,null,null,null,null,"<DateFormat>dd-MM-yyyy hh:mm:ss</DateFormat> "]
[null,null,null,null,"      <BaseID>205</BaseID>",null,null,null,null,null,null,null,null,null,null,"<DateValueElements>"]
[null,null,null,null,"      <DataName>Elspot</DataName>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"01-01-2009 00:00:00\" Value=\"27.56\"></Data>"]
[null,null,null,null,"      <DataElementName>weatherdata.TimeSeries</DataElementName>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"01-01-2009 06:00:00:00\" Value=\"0.81\"></Data>"]
[null,null,null,null,"      <TimeSeriesFileName>c:\\ePxml\\ElspotVestdanmark2009.epw</TimeSeriesFileName>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"01-01-2009 21:00:00\" Value=\"0.56\"></Data>"]
[null,null,null,null,"      <TimeSeriesFileType>epw</TimeSeriesFileType>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"02-01-2009\" Value=\"34.65\"></Data>"]
[null,null,null,null,"   </InputDataElement>",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"02-01-2009 06\" Value=\"38.81\"></Data>"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"02-01-08 21:00:00\" Value=\"34.65\"></Data>"]
[null,null,null,null,"csv:",null,null,null,null,null,null,null,null,null,null,null,"<Data Time=\"03-01-2009 00:00:00\" Value=\"31.19\"></Data>"]
[null,null,null,null,"    <InputDataElement>      ",null,null,null,null,null,null,null,null,null,null," </DateValueElements>"]
[null,null,null,null,"      <BaseID>205</BaseID>",null,null,null,null,null,null,null,null,null,"</TimeSeriesElement> "]
[null,null,null,null,"      <DataName>Elspot</DataName>",null,null,null,null,null,null,null,null,null,"  </ePROTimeSeriesData>"]
[null,null,null,null,"      <DataElementName>weatherdata.TimeSeries</DataElementName>"]
[null,null,null,null,"      <ReportDelimiter>;</ReportDelimiter>"]
[null,null,null,null,"      <TimeSeriesFileName>c:\\ePxml\\Elspot2011.csv</TimeSeriesFileName>"]
[null,null,null,null,"      <TimeSeriesFileType>csv</TimeSeriesFileType>"]
[null,null,null,null,"   </InputDataElement>"]
[]
["Demand"]
[null,"DaylyRatioFormular",null,null,"Modifying annual heat demand"]
[null,"Demand",null,null,"   <InputDataElement> "]
[null,"DemandFrom",null,null,null,"<BaseID>500</BaseID> "]
[null,"DemandTo",null,null,null,"<DataName>Heat Demand</DataName> "]
[null,"IncludedFrom",null,null,null,"<DataElementName>Demand</DataElementName> "]
[null,"IncludedTo",null,null,null,"<DataElementValue>99999</DataElementValue> "]
[null,"OutDoorTempSymbol",null,null,"   </InputDataElement> "]
[null,"ReferenceTemperature"]
[null,"SiteID",null,null,"Modifying weather dependency fraction:"]
[null,"WeatherDepFraction",null,null,"   <InputDataElement> "]
[null,"WeatherDepSeasonFrom",null,null,null,"<BaseID>500</BaseID> "]
[null,"WeatherDepSeasonTo",null,null,null,"<DataName>Heat Demand</DataName> "]
[null,null,null,null,null,"<DataElementName>WeatherDepFraction</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>23</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
[null,null,null,null,"Demand as time series:"]
[null,null,null,null,"   <InputDataElement>      "]
[null,null,null,null,null,"<BaseID>500</BaseID>"]
[null,null,null,null,null,"<DataName>HeatDemand</DataName>"]
[null,null,null,null,null,"<DataElementName>weatherdata.TimeSeries</DataElementName>"]
[null,null,null,null,null,"<TimeSeriesFileName>c:\\temp\\xmltest\\HeatDemand.epw</TimeSeriesFileName>"]
[null,null,null,null,null,"<TimeSeriesFileType>epw</TimeSeriesFileType>"]
[null,null,null,null,"   </InputDataElement>"]
[]
["Fuels"]
[null,"FuelContentPrimo",null,null,"content of fuel store primo calculation"]
[null,"FuelContentUltimo",null,null," <InputDataElement> "]
[null,"FuelStorage",null,null,null,"<BaseID>400</BaseID> "]
[null,"ThermalValue",null,null,null,"<DataName>Naturgas</DataName> "]
[null,"UnitName",null,null,null,"<DataElementName>FuelContentPrimo</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>17</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[null,null,null,null,"content of fuel store ultimo of calculation"]
[null,null,null,null,"   <InputDataElement> "]
[null,null,null,null,null,"<BaseID>400</BaseID> "]
[null,null,null,null,null,"<DataName>Naturgas</DataName> "]
[null,null,null,null,null,"<DataElementName>FuelContentUltimo</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>21</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
["Energy conversion units"]
[null,"NonOperTimes",null,null,"Start of first non operation period"]
[null,"OperationalFrom",null,null,"<InputDataElement>"]
[null,"OperationalTo",null,null,null,"<BaseID>600</BaseID>"]
[null,"PowerCurve",null,null,null,"<DataName>Motor1</DataName>"]
[null,"ShutDownPeriod",null,null,null,"<DataElementName>NonOperTimes.StartTime</DataElementName>"]
[null,"SolarUnit",null,null,null,"<DataElementIndex>1</DataElementIndex>"]
[null,"StartUpPeriod",null,null,null,"<DataElementTimeValue>01-01-2012 12:00</DataElementTimeValue>"]
[null,"WindFarm",null,null,"</InputDataElement>"]
[]
[null,"PowerCurve:",null,null,"End of first non operation period"]
[null,"CoolProd",null,null,"<InputDataElement>"]
[null,"ElCon",null,null,null,"<BaseID>600</BaseID>"]
[null,"ElProd",null,null,null,"<DataName>Motor1</DataName>"]
[null,"Fuel",null,null,null,"<DataElementName>NonOperTimes.EndTime</DataElementName>"]
[null,"HeatCon",null,null,null,"<DataElementIndex>1</DataElementIndex>"]
[null,"HeatProd",null,null,null,"<DataElementTimeValue>02-01-2012 17:00</DataElementTimeValue>"]
[null,"ProcHeatCon",null,null,"</InputDataElement>"]
[null,"ProcHeatProd"]
[null,null,null,null,"Power curve value"]
[null,"SolarUnit:",null,null,"<InputDataElement>"]
[null,"IncidenceAngleMod50",null,null,null,"<BaseID>600</BaseID>"]
[null,"IncidenceAngleModCoef",null,null,null,"<DataName>Motor1</DataName>"]
[null,"IncidenceAngleModSavedAsCoeff",null,null,null,"<DataElementName>PowerCurve.Fuel</DataElementName>"]
[null,"Inclination",null,null,null,"<DataElementValue>3669</DataElementValue>"]
[null,"InstalledElecCapacity",null,null,"</InputDataElement>"]
[null,"K0"]
[null,"K1",null,null,"Solar collector area"]
[null,"Lattitude",null,null,"<InputDataElement>"]
[null,"N0",null,null,null,"<BaseID>600</BaseID>"]
[null,"NOCT",null,null,null,"<DataName>Solfanger</DataName>"]
[null,"Orientation",null,null,null,"<DataElementName>SolarUnit.TotalArea</DataElementName>"]
[null,"PMax",null,null,null,"<DataElementValue>9876</DataElementValue>"]
[null,"PowerLosses",null,null,"</InputDataElement>"]
[null,"ReflectionFactor"]
[null,"TempCoeffPower"]
[null,"TemperatureAvg"]
[null,"TotalArea"]
[]
[null,"WindFarm"]
[null,"AnnualProduction"]
[null,"Conversiontable"]
[null,"HellmannExp"]
[null,"HubHeight"]
[null,"MeasureHeight"]
[null,"ScaleType"]
[null,"ScaleValue"]
[null,"WindFarmCalcType"]
[null,"WindTSID"]
[]
[]
["Stores"]
[null,"PrimoStorage",null,null,"Storage content, start"]
[null,"StorageUtilization",null,null,"   <InputDataElement> "]
[null,"UltimoStorage",null,null,null,"<BaseID>650</BaseID> "]
[null,null,null,null,null,"<DataName>Varmelager</DataName> "]
[null,null,null,null,null,"<DataElementName>PrimoStorage</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>11</DataElementValue> "]
[null,null,null,null,"   </InputDataElement> "]
[]
[null,null,null,null,"Storage content, end"]
[null,null,null,null,null,"<BaseID>650</BaseID> "]
[null,null,null,null,null,"<DataName>Varmelager</DataName> "]
[null,null,null,null,null,"<DataElementName>UltimoStorage</DataElementName> "]
[null,null,null,null,null,"<DataElementValue>12</DataElementValue> "]
[null,null,null,null,"   </InputDataElement>"]
[]
["Payments"]
[null,"Amount",null,null,"Amount (price per unit):"]
[null,null,null,null,"    <InputDataElement>      "]
[null,null,null,null,null,"      <BaseID>800</BaseID>"]
[null,null,null,null,null,"      <DataName>NOx-afgifter.Motor 1</DataName>"]
[null,null,null,null,null,"      <DataElementName>amount</DataElementName>"]
[null,null,null,null,null,"      <DataElementValue>0.03</DataElementValue> "]
[null,null,null,null,"   </InputDataElement>"]
[]
["Reports"]
[null,null,null,null,"Energy conversion, annual:"]
[null,null,null,null,"   <OutputDataElement>      "]
[null,null,null,null,"      <ReportBaseID>200</ReportBaseID>"]
[null,null,null,null,"      <ReportDelimiter>;</ReportDelimiter>"]
[null,null,null,null,"      <ReportFileName>c:\\Energy conversion, annual.txt</ReportFileName>"]
[null,null,null,null,"      <ReportFileType>txt</ReportFileType>"]
[null,null,null,null,"   </OutputDataElement>   "]
[]
[null,null,null,null,"Production, graphic:"]
[null,null,null,null,"   <OutputDataElement>      "]
[null,null,null,null,"      <ReportBaseID>100</ReportBaseID>"]
[null,null,null,null,"      <ReportFileName>c:\\production, graphic1.jpg</ReportFileName>"]
[null,null,null,null,"      <ReportFileType>jpg</ReportFileType>"]
[null,null,null,null,"      <ReportStartDate>15-07-2011 00:00</ReportStartDate>"]
[null,null,null,null,"      <ReportEndDate>23-07-2011 00:00</ReportEndDate>"]
[null,null,null,null,"   </OutputDataElement>   "]
[]
[null,null,null,null,"Operation Income:"]
[null,null,null,null,"   <OutputDataElement>      "]
[null,null,null,null,"      <ReportBaseID>10030</ReportBaseID>"]
[null,null,null,null,"      <ReportDelimiter>;</ReportDelimiter>"]
[null,null,null,null,"      <ReportFileName>c:\\OperationIncome.csv</ReportFileName>"]
[null,null,null,null,"      <ReportFileType>csv</ReportFileType>"]
[null,null,null,null,"   </OutputDataElement>   "]